## SPI Registers

Register Name | Register Description | Address
--- | --- | ---
SPI0_CFG | SPI Configuration Register | 0x40000B00
SPI0_CTRL | SPI Control Register | 0x40000B04
SPI0_STATUS | SPI Status Register | 0x40000B08
SPI0_TX_DATA | SPI Transmit Data Register | 0x40000B0C
SPI0_RX_DATA | SPI Received Data Register | 0x40000B10
SPI0_RX_DATA_NO_START | SPI Received Data No Start Register | 0x40000B14
SPI0_RX_DATA_MIRROR | SPI Received Data Mirror Register | 0x40000B18
SPI0_ID_NUM | SPI ID number | 0x40000BFC
SPI1_CFG | SPI Configuration Register | 0x40000C00
SPI1_CTRL | SPI Control Register | 0x40000C04
SPI1_STATUS | SPI Status Register | 0x40000C08
SPI1_TX_DATA | SPI Transmit Data Register | 0x40000C0C
SPI1_RX_DATA | SPI Received Data Register | 0x40000C10
SPI1_RX_DATA_NO_START | SPI Received Data No Start Register | 0x40000C14
SPI1_RX_DATA_MIRROR | SPI Received Data Mirror Register | 0x40000C18
SPI1_ID_NUM | SPI ID number | 0x40000CFC