### BB_RADIOPWRUPDN3

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
14:8 | RW | TXPWRDN3 | Radio Tx power down (in us) for coded PHY at 500kbps
7:0 | RW | TXPWRUP3 | Radio Tx power up for (in us) PHY at 500kbps

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
14:8 | TXPWRDN3 | TXPWRDN3_0 |  | 0x0*
7:0 | TXPWRUP3 | TXPWRUP3_0 |  | 0x0*