### ACS_RTC_COUNT_THRES

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:0 | RW | THRESHOLD | Compare value for the RTC counter

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:0 | THRESHOLD | RTC_COUNT_THRES_0 | Compare to 0 | 0x0
|  | RTC_COUNT_THRES_1 | Compare to 1 | 0x1
|  | RTC_COUNT_THRES_32767 | Compare to 32,767 | 0x7FFF
|  | RTC_COUNT_THRES_4294967295 | Compare to 4,294,967,295 | 0xFFFFFFFF*