### RF_TX_PULSE_SHAPE_1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_PULSE_SHAPE_1_TX_COEF4 | Tx pulse shape coefficient 4 (banked)
23:16 | RW | TX_PULSE_SHAPE_1_TX_COEF3 | Tx pulse shape coefficient 3 (banked)
15:8 | RW | TX_PULSE_SHAPE_1_TX_COEF2 | Tx pulse shape coefficient 2 (banked)
7:0 | RW | TX_PULSE_SHAPE_1_TX_COEF1 | Tx pulse shape coefficient 1 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_PULSE_SHAPE_1_TX_COEF4 | TX_PULSE_SHAPE_1_TX_COEF4_DEFAULT |  | 0x0*
23:16 | TX_PULSE_SHAPE_1_TX_COEF3 | TX_PULSE_SHAPE_1_TX_COEF3_DEFAULT |  | 0x0*
15:8 | TX_PULSE_SHAPE_1_TX_COEF2 | TX_PULSE_SHAPE_1_TX_COEF2_DEFAULT |  | 0x0*
7:0 | TX_PULSE_SHAPE_1_TX_COEF1 | TX_PULSE_SHAPE_1_TX_COEF1_DEFAULT |  | 0x0*