### RF_TX_PULSE_SHAPE_2

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_PULSE_SHAPE_2_TX_COEF8 | Tx pulse shape coefficient 8 (banked)
23:16 | RW | TX_PULSE_SHAPE_2_TX_COEF7 | Tx pulse shape coefficient 7 (banked)
15:8 | RW | TX_PULSE_SHAPE_2_TX_COEF6 | Tx pulse shape coefficient 6 (banked)
7:0 | RW | TX_PULSE_SHAPE_2_TX_COEF5 | Tx pulse shape coefficient 5 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_PULSE_SHAPE_2_TX_COEF8 | TX_PULSE_SHAPE_2_TX_COEF8_DEFAULT |  | 0x2*
23:16 | TX_PULSE_SHAPE_2_TX_COEF7 | TX_PULSE_SHAPE_2_TX_COEF7_DEFAULT |  | 0x1*
15:8 | TX_PULSE_SHAPE_2_TX_COEF6 | TX_PULSE_SHAPE_2_TX_COEF6_DEFAULT |  | 0x0*
7:0 | TX_PULSE_SHAPE_2_TX_COEF5 | TX_PULSE_SHAPE_2_TX_COEF5_DEFAULT |  | 0x0*