# Memory Registers

Register Name | Register Description | Address
--- | --- | ---
SYSCTRL_CM33_LOOP_CACHE_CFG | CM33 Loop Cache Configuration | 0x40000000
SYSCTRL_ACCESS_ERROR | Memory and Peripheral Access Error Flags | 0x40000004
SYSCTRL_MEM_POWER_STARTUP | Memory Power Configuration | 0x40000008
SYSCTRL_MEM_POWER_ENABLE | Memory Power Configuration | 0x4000000C
SYSCTRL_MEM_ACCESS_CFG | Memory Access Configuration and wake-up Restore Address in packed 4-bit format | 0x40000018
SYSCTRL_WAKEUP_ADDR | Wake-up Restore Address in Unpacked 32-bit Format | 0x4000001C
SYSCTRL_MEM_RETENTION_CFG | Memory Retention Configuration | 0x40000020
SYSCTRL_MEM_TIMING_CFG | Memory Timing Configuration | 0x40000024