### BB_DEBUGADDMAX

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:16 | RW | REG_ADDMAX | Upper limit for the register zone indicated by the reg_inzone flag
15:0 | RW | EM_ADDMAX | Upper limit for the exchange memory zone indicated by the em_inzone flag

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:16 | REG_ADDMAX | REG_ADDMAX_0 |  | 0x0*
15:0 | EM_ADDMAX | EM_ADDMAX_0 |  | 0x0*