### RF_RX_PULSE_SHAPE

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | RX_PULSE_SHAPE_RX_COEF8 | Rx pulse shape coefficient 8 (banked)
27:24 | RW | RX_PULSE_SHAPE_RX_COEF7 | Rx pulse shape coefficient 7 (banked)
23:20 | RW | RX_PULSE_SHAPE_RX_COEF6 | Rx pulse shape coefficient 6 (banked)
19:16 | RW | RX_PULSE_SHAPE_RX_COEF5 | Rx pulse shape coefficient 5 (banked)
15:12 | RW | RX_PULSE_SHAPE_RX_COEF4 | Rx pulse shape coefficient 4 (banked)
11:8 | RW | RX_PULSE_SHAPE_RX_COEF3 | Rx pulse shape coefficient 3 (banked)
7:4 | RW | RX_PULSE_SHAPE_RX_COEF2 | Rx pulse shape coefficient 2 (banked)
3:0 | RW | RX_PULSE_SHAPE_RX_COEF1 | Rx pulse shape coefficient 1 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:28 | RX_PULSE_SHAPE_RX_COEF8 | RX_PULSE_SHAPE_RX_COEF8_DEFAULT |  | 0xF*
27:24 | RX_PULSE_SHAPE_RX_COEF7 | RX_PULSE_SHAPE_RX_COEF7_DEFAULT |  | 0xE*
23:20 | RX_PULSE_SHAPE_RX_COEF6 | RX_PULSE_SHAPE_RX_COEF6_DEFAULT |  | 0xC*
19:16 | RX_PULSE_SHAPE_RX_COEF5 | RX_PULSE_SHAPE_RX_COEF5_DEFAULT |  | 0xA*
15:12 | RX_PULSE_SHAPE_RX_COEF4 | RX_PULSE_SHAPE_RX_COEF4_DEFAULT |  | 0x7*
11:8 | RX_PULSE_SHAPE_RX_COEF3 | RX_PULSE_SHAPE_RX_COEF3_DEFAULT |  | 0x4*
7:4 | RX_PULSE_SHAPE_RX_COEF2 | RX_PULSE_SHAPE_RX_COEF2_DEFAULT |  | 0x2*
3:0 | RX_PULSE_SHAPE_RX_COEF1 | RX_PULSE_SHAPE_RX_COEF1_DEFAULT |  | 0x1*