### SENSOR_PROCESSING

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24 | RW | SUM_EN | Summation enable
19:16 | RW | NBR_SAMPLES | Number of samples used for wakeup in sensor detect mode

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24 | SUM_EN | SENSOR_SUMMATION_DISABLED | Summation is disabled | 0x0*
|  | SENSOR_SUMMATION_ENABLED | Summation is enabled | 0x1
19:16 | NBR_SAMPLES | SENSOR_NBR_SAMPLES_1 | 1 sample used | 0x0*
|  | SENSOR_NBR_SAMPLES_2 | 2 samples used | 0x1
|  | SENSOR_NBR_SAMPLES_16 | 16 samples used | 0xF