### SYSCTRL_CNT_CTRL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
3 | R | CNT_STATUS | Activity counters status bit
2 | W | CNT_CLEAR | Clear activity counters
1 | W | CNT_STOP | Stop activity counters
0 | W | CNT_START | Start activity counters

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
3 | CNT_STATUS | CNT_STOPPED | Activity counters stopped | 0x0*
|  | CNT_RUNNING | Activity counters running | 0x1
2 | CNT_CLEAR | CNT_CLEAR | Clear activity counters | 0x1
1 | CNT_STOP | CNT_STOP | Stop activity counters | 0x1
0 | CNT_START | CNT_START | Start activity counters | 0x1