### RF_TX_PULSE_SHAPE_4

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_PULSE_SHAPE_4_TX_COEF16 | Tx pulse shape coefficient 16 (banked)
23:16 | RW | TX_PULSE_SHAPE_4_TX_COEF15 | Tx pulse shape coefficient 15 (banked)
15:8 | RW | TX_PULSE_SHAPE_4_TX_COEF14 | Tx pulse shape coefficient 14 (banked)
7:0 | RW | TX_PULSE_SHAPE_4_TX_COEF13 | Tx pulse shape coefficient 13 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_PULSE_SHAPE_4_TX_COEF16 | TX_PULSE_SHAPE_4_TX_COEF16_DEFAULT |  | 0x7D*
23:16 | TX_PULSE_SHAPE_4_TX_COEF15 | TX_PULSE_SHAPE_4_TX_COEF15_DEFAULT |  | 0x75*
15:8 | TX_PULSE_SHAPE_4_TX_COEF14 | TX_PULSE_SHAPE_4_TX_COEF14_DEFAULT |  | 0x66*
7:0 | TX_PULSE_SHAPE_4_TX_COEF13 | TX_PULSE_SHAPE_4_TX_COEF13_DEFAULT |  | 0x4F*