### BB_ACTSCANCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
24:16 | RW | BACKOFF | Active scan mode back-off counter initialization value
8:0 | RW | UPPERLIMIT | Active scan mode upper limit counter value

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
24:16 | BACKOFF | BACKOFF_1 |  | 0x1*
8:0 | UPPERLIMIT | UPPERLIMIT_1 |  | 0x1*