### FPE_MVFR0

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:28 | RW | FPROUND | All rounding modes supported
23:20 | RW | FPSQRT | Floating-point square root
19:16 | RW | FPDIVIDE | Floating-point divide
11:8 | RW | FPDP | Floating-point double-precision
7:4 | RW | FPSP | Floating-point single-precision
3:0 | RW | SIMDREG | SIMD registers. Indicates size of floating-point extension register file. (15*64 bit registers)