## NVIC Registers

NOTE: Individual register tables are not included for the _NS registers listed here, as the registers are all identical except for their offsets. For more information, see TrustZone.

Register Name | Register Description | Address
--- | --- | ---
NVIC_ISER0 | NVIC External Interrupt Set Enable Register 0 | 0xE000E100
NVIC_ISER1 | NVIC External Interrupt Set Enable Register 1 | 0xE000E104
NVIC_ICER0 | NVIC External Interrupt Clear Enable Register 0 | 0xE000E180
NVIC_ICER1 | NVIC External Interrupt Clear Enable Register 1 | 0xE000E184
NVIC_ISPR0 | NVIC External Interrupt Set Pending Register 0 | 0xE000E200
NVIC_ISPR1 | NVIC External Interrupt Set Pending Register 1 | 0xE000E204
NVIC_ICPR0 | NVIC External Interrupt Clear Pending Register 0 | 0xE000E280
NVIC_ICPR1 | NVIC External Interrupt Clear Pending Register 1 | 0xE000E284
NVIC_IABR0 | NVIC External Interrupt Active Register 0 | 0xE000E300
NVIC_IABR1 | NVIC External Interrupt Active Register 1 | 0xE000E304
NVIC_ITNS0 | NVIC External Interrupt Non-secure Register 0 | 0xE000E380
NVIC_ITNS1 | NVIC External Interrupt Non-secure Register 1 | 0xE000E384
NVIC_IPR0 | NVIC External Interrupt Priority Register 0 | 0xE000E400
NVIC_IPR1 | NVIC External Interrupt Priority Register 1 | 0xE000E404
NVIC_IPR2 | NVIC External Interrupt Priority Register 2 | 0xE000E408
NVIC_IPR3 | NVIC External Interrupt Priority Register 3 | 0xE000E40C
NVIC_IPR4 | NVIC External Interrupt Priority Register 4 | 0xE000E410
NVIC_IPR5 | NVIC External Interrupt Priority Register 5 | 0xE000E414
NVIC_IPR6 | NVIC External Interrupt Priority Register 6 | 0xE000E418
NVIC_IPR7 | NVIC External Interrupt Priority Register 7 | 0xE000E41C
NVIC_IPR8 | NVIC External Interrupt Priority Register 8 | 0xE000E420
NVIC_IPR9 | NVIC External Interrupt Priority Register 9 | 0xE000E424
NVIC_IPR10 | NVIC External Interrupt Priority Register 10 | 0xE000E428
NVIC_IPR11 | NVIC External Interrupt Priority Register 11 | 0xE000E42C
NVIC_IPR12 | NVIC External Interrupt Priority Register 12 | 0xE000E430
NVIC_IPR13 | NVIC External Interrupt Priority Register 13 | 0xE000E434
NVIC_IPR14 | NVIC External Interrupt Priority Register 14 | 0xE000E438
NVIC_ISER0_NS | NVIC External Interrupt Set Enable Register 0 | 0xE002E100
NVIC_ISER1_NS | NVIC External Interrupt Set Enable Register 1 | 0xE002E104
NVIC_ICER0_NS | NVIC External Interrupt Clear Enable Register 0 | 0xE002E180
NVIC_ICER1_NS | NVIC External Interrupt Clear Enable Register 1 | 0xE002E184
NVIC_ISPR0_NS | NVIC External Interrupt Set Pending Register 0 | 0xE002E200
NVIC_ISPR1_NS | NVIC External Interrupt Set Pending Register 1 | 0xE002E204
NVIC_ICPR0_NS | NVIC External Interrupt Clear Pending Register 0 | 0xE002E280
NVIC_ICPR1_NS | NVIC External Interrupt Clear Pending Register 1 | 0xE002E284
NVIC_IABR0_NS | NVIC External Interrupt Active Register 0 | 0xE002E300
NVIC_IABR1_NS | NVIC External Interrupt Active Register 1 | 0xE002E304
NVIC_IPR0_NS | NVIC External Interrupt Priority Register 0 | 0xE002E400
NVIC_IPR1_NS | NVIC External Interrupt Priority Register 1 | 0xE002E404
NVIC_IPR2_NS | NVIC External Interrupt Priority Register 2 | 0xE002E408
NVIC_IPR3_NS | NVIC External Interrupt Priority Register 3 | 0xE002E40C
NVIC_IPR4_NS | NVIC External Interrupt Priority Register 4 | 0xE002E410
NVIC_IPR5_NS | NVIC External Interrupt Priority Register 5 | 0xE002E414
NVIC_IPR6_NS | NVIC External Interrupt Priority Register 6 | 0xE002E418
NVIC_IPR7_NS | NVIC External Interrupt Priority Register 7 | 0xE002E41C
NVIC_IPR8_NS | NVIC External Interrupt Priority Register 8 | 0xE002E420
NVIC_IPR9_NS | NVIC External Interrupt Priority Register 9 | 0xE002E424
NVIC_IPR10_NS | NVIC External Interrupt Priority Register 10 | 0xE002E428
NVIC_IPR11_NS | NVIC External Interrupt Priority Register 11 | 0xE002E42C
NVIC_IPR12_NS | NVIC External Interrupt Priority Register 12 | 0xE002E430
NVIC_IPR13_NS | NVIC External Interrupt Priority Register 13 | 0xE002E434
NVIC_IPR14_NS | NVIC External Interrupt Priority Register 14 | 0xE002E538