### CLK_DIV_CFG1

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
27 | RW | SENSOR_CLK_DISABLE | Sensor clock disable
26:16 | RW | SENSOR_CLK_PRESCALE | Prescale value for the sensor clock
15 | RW | CPCLK_DISABLE | Charge pump clock disable
13:8 | RW | CPCLK_PRESCALE | Prescale value for the charge pump clock from the SLOWCLK clock (1 to 64 in steps of 1)
7 | RW | DCCLK_DISABLE | DC-DC converter clock disable
5:0 | RW | DCCLK_PRESCALE | Prescale value for the DC-DC converter clock (1 to 64 in steps of 1)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
27 | SENSOR_CLK_DISABLE | SENSOR_CLK_ENABLE | Sensor clock enabled | 0x0
|  | SENSOR_CLK_DISABLE | Sensor clock disabled | 0x1*
26:16 | SENSOR_CLK_PRESCALE | SENSOR_PRESCALE_1 | Divide by 1 | 0x0*
|  | SENSOR_PRESCALE_2 | Divide by 2 | 0x1
|  | SENSOR_PRESCALE_3 | Divide by 3 | 0x2
|  | SENSOR_PRESCALE_1464 | Divide by 1464 | 0x5B8
|  | SENSOR_PRESCALE_1465 | Divide by 1465 | 0x5B9
|  | SENSOR_PRESCALE_1466 | Divide by 1466 | 0x5BA
|  | SENSOR_PRESCALE_2046 | Divide by 2046 | 0x7FD
|  | SENSOR_PRESCALE_2047 | Divide by 2047 | 0x7FE
|  | SENSOR_PRESCALE_2048 | Divide by 2048 | 0x7FF
15 | CPCLK_DISABLE | CPCLK_ENABLE | Charge pump clock enabled | 0x0*
|  | CPCLK_DISABLE | Charge pump clock disabled | 0x1
13:8 | CPCLK_PRESCALE | CPCLK_PRESCALE_1 | Divide by 1 | 0x0
|  | CPCLK_PRESCALE_2 | Divide by 2 | 0x1
|  | CPCLK_PRESCALE_3 | Divide by 3 | 0x2
|  | CPCLK_PRESCALE_4 | Divide by 4 | 0x3
|  | CPCLK_PRESCALE_5 | Divide by 5 | 0x4
|  | CPCLK_PRESCALE_6 | Divide by 6 | 0x5
|  | CPCLK_PRESCALE_7 | Divide by 7 | 0x6
|  | CPCLK_PRESCALE_8 | Divide by 8 | 0x7*
|  | CPCLK_PRESCALE_9 | Divide by 9 | 0x8
|  | CPCLK_PRESCALE_10 | Divide by 10 | 0x9
|  | CPCLK_PRESCALE_63 | Divide by 63 | 0x3E
|  | CPCLK_PRESCALE_64 | Divide by 64 | 0x3F
7 | DCCLK_DISABLE | DCCLK_ENABLE | DC-DC converter clock enabled | 0x0*
|  | DCCLK_DISABLE | DC-DC converter clock disabled | 0x1
5:0 | DCCLK_PRESCALE | DCCLK_PRESCALE_1 | Divide by 1 | 0x0*
|  | DCCLK_PRESCALE_2 | Divide by 2 | 0x1
|  | DCCLK_PRESCALE_3 | Divide by 3 | 0x2
|  | DCCLK_PRESCALE_4 | Divide by 4 | 0x3
|  | DCCLK_PRESCALE_5 | Divide by 5 | 0x4
|  | DCCLK_PRESCALE_6 | Divide by 6 | 0x5
|  | DCCLK_PRESCALE_7 | Divide by 7 | 0x6
|  | DCCLK_PRESCALE_8 | Divide by 8 | 0x7
|  | DCCLK_PRESCALE_9 | Divide by 9 | 0x8
|  | DCCLK_PRESCALE_10 | Divide by 10 | 0x9
|  | DCCLK_PRESCALE_12 | Divide by 12 | 0xB
|  | DCCLK_PRESCALE_63 | Divide by 63 | 0x3E
|  | DCCLK_PRESCALE_64 | Divide by 64 | 0x3F