### RF_TX_PULSE_SHAPE_3

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
31:24 | RW | TX_PULSE_SHAPE_3_TX_COEF12 | Tx pulse shape coefficient 12 (banked)
23:16 | RW | TX_PULSE_SHAPE_3_TX_COEF11 | Tx pulse shape coefficient 11 (banked)
15:8 | RW | TX_PULSE_SHAPE_3_TX_COEF10 | Tx pulse shape coefficient 10 (banked)
7:0 | RW | TX_PULSE_SHAPE_3_TX_COEF9 | Tx pulse shape coefficient 9 (banked)

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
31:24 | TX_PULSE_SHAPE_3_TX_COEF12 | TX_PULSE_SHAPE_3_TX_COEF12_DEFAULT |  | 0x36*
23:16 | TX_PULSE_SHAPE_3_TX_COEF11 | TX_PULSE_SHAPE_3_TX_COEF11_DEFAULT |  | 0x20*
15:8 | TX_PULSE_SHAPE_3_TX_COEF10 | TX_PULSE_SHAPE_3_TX_COEF10_DEFAULT |  | 0x10*
7:0 | TX_PULSE_SHAPE_3_TX_COEF9 | TX_PULSE_SHAPE_3_TX_COEF9_DEFAULT |  | 0x7*