### BB_TIMGENCNTL

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
25:16 | RW | PREFETCHABORT_TIME | Define the instant in us at which immediate abort is required after anticipated pre-fetch abort
8:0 | RW | PREFETCH_TIME | Define exchange table pre-fetch instant in us

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
25:16 | PREFETCHABORT_TIME | PREFETCHABORT_TIME_254 |  | 0x1FE*
8:0 | PREFETCH_TIME | PREFETCH_TIME_150 |  | 0x96*