### LIN_CFG

Bit Field | Read/Write | Field Name | Description
--- | --- | --- | ---
8 | RW | CHECKSUM_MODE | Select checksum mode
4 | RW | INIT | Start C617 initialization
0 | R | STANDBY | C617 state

Bit Field | Field Name | Value Symbol | Value Description | Hex Value
--- | --- | --- | --- | ---
8 | CHECKSUM_MODE | ID_IN_CHECKSUM | Enhance check sum, include ID | 0x0*
|  | ONLY_DATA_IN_CHECKSUM | Classic check sum, only data byte | 0x1
4 | INIT | NOT_INIT_C617 |  | 0x0*
|  | INIT_C617 |  | 0x1
0 | STANDBY | STANDBY_STATE |  | 0x0*
|  | NORMAL_MODE |  | 0x1